高中生物必修1知识点总结
1、生命系统的结构层次依次为:细胞?组织?器官?系统?个体?种群?群落?生态系统 
细胞是生物体结构和功能的基本单位;地球上最基本的生命系统是细胞 2、光学显微镜的操作步骤:对光?低倍物镜观察?移动视野中央(偏哪移哪)?高倍物镜观察:?只能调节细准焦螺旋;?调节大光圈、凹面镜 ?3、原核细胞与真核细胞根本区别为:有无核膜为界限的细胞核 ?原核细胞:无核膜，无染色体，如大肠杆菌等细菌、蓝藻 
?真核细胞:有核膜，有染色体，如酵母菌，各种动物 
注:病毒无细胞结构，但有DNA或RNA 
4、蓝藻是原核生物，自养生物 
、真核细胞与原核细胞统一性体现在二者均有细胞膜和细胞质 5
6、细胞学说建立者是施莱登和施旺，细胞学说建立揭示了细胞的统一性和生物体结构的统 
一性。细胞学说建立过程，是一个在科学探究中开拓、继承、修正和发展的过程，充满耐人寻味的曲折 
7、组成细胞(生物界)和无机自然界的化学元素种类大体相同，含量不同 ?8、组成细胞的元素 
?大量无素:C、H、O、N、P、S、K、Ca、Mg 
?微量无素:Fe、Mn、B、Zn、Mo、Cu 
?主要元素:C、H、O、N、P、S 
?基本元素:C 
?细胞干重中，含量最多元素为C，鲜重中含最最多元素为O ?9、生物(如沙漠中仙人掌)鲜重中，含量最多化合物为水，干重中含量最多的化合物为蛋白质。 
?10、(1)还原糖(葡萄糖、果糖、麦芽糖)可与斐林试剂反应生成砖红色沉淀;脂肪可苏丹III染成橘黄色(或被苏丹IV染成红色);淀粉(多糖)遇碘变蓝色;蛋白质与双缩脲试剂产生紫色反应。(2)还原糖鉴定材料不能选用甘ensure that backfill compacting. 6.4.2 construction safety construction project since there are more heavy equipment for construction, construction must pay attention to security. Construction will earnestly implement the employer's company, supervising engineer of construction-related safety instructions, requirements, and improve safe operation of safe and civilized construction management and technology. (1) the construction vehicle, loader, backhoe and other heavy machinery and equipment maintenance as required to ensure the machine normal use. (2) Dumper filling face discharge, arrange command to avoid crash when reversing. (3) the bulldozed filling arrangement has some experience of the pilot and construction. 6.5 filling main equipment table of main construction equipment serial number name model units number remark 1 hydraulic excavator with backhoe loading and unloading truck 5T CAT320 3 2 8 3 wheel loader L30 3 4 loader ... 7.2.7 pressure concrete penstock in construction of concrete-filled steel tube concrete mixing truck transported horizontally HB60 direct placement of concrete delivery pump or chute directly from top to bottom in the granary, manual open, φ 38~ 50mm shaft for electric vibrating needle vibrated. Begin within 12~18h
 after finishing maintenance. Maintenance keep the mulch cover, protection of water saturation. 7.2.8 construction of hoist room-and-pillar method of concrete construction using layered construction from the bottom up, layer thickness 2.4m. Roof template uses the template of standard steel assembling, corner parts using small pieces of steel or wooden template, the template is used in 48mm steel pipe erection full House scaffolding support. Steel in steel processing processing is completed, transport by trucks to the construction site, then H30B perpendicular to the face of the tower crane, artificial binding welded. Concrete by tanker transport to the pier HB60 direct placement of concrete delivery pump, manual open, 38mm shaft for electric plug-in vibrator vibrating compaction. 7.3 7.3.1 in concrete construction of concrete (1) cement-cement construction drawings of buildings according to the requirements, configure the required cement concrete, cement in accordance with existing national and industry standards. Ship each batch of cement factory, on cement quality, factory certificate, review the information for inspection re-inspection. Transport of cement in the transport process, the different varieties and different levels of intensity may not be mixed, and to take measures to prevent the cement from moisture. Storage delivery of cement according to the variety, intensity, the factory lot, bagged or in bulk, respectively, kept in its own warehouses or storage tank to prevent cement deterioration. Bags of cement manufacture date not more than 3 months, bulk cement factory date not more 
蔗(3)斐林试剂必须现配现用(与双缩脲试剂不同，双缩脲试剂先加A液，再加B液)R 
?11、蛋白质的基本组成单位是氨基酸，氨基酸结构通式为NH2—C—COOH，各种氨基酸的区别在于R基的不同。 
?12、两个氨基酸脱水缩合形成二肽，连接两个氨基酸分子的化学键(—NH—CO—)叫肽键。 
?13、脱水缩合中，脱去水分子数=形成的肽键数=氨基酸数—肽链条数 ?14、蛋白质多样性原因:构成蛋白质的氨基酸种类、数目、排列顺序千变万化，多肽链盘曲折叠方式千差万别。 
?15、每种氨基酸分子至少都含有一个氨基(—NH2)和一个羧基(—COOH)，并且都有一个氨基和一个羧基连接在同一个碳原子上，这个碳原子还连接一个氢原子和一个侧链基因。 
?16、遗传信息的携带者是核酸，它在生物体的遗传变异和蛋白质合成中具有极其重要作用，核酸包括两大类:一类是脱氧核糖核酸，简称DNA;一类是核糖核酸，简称RNA，核酸基本组成单位核苷酸。 
17、蛋白质功能: 
?结构蛋白，如肌肉、羽毛、头发、蛛丝 
?催化作用，如绝大多数酶 
?运输载体，如血红蛋白 
?传递信息，如胰岛素 
?免疫功能，如抗体 
18、氨基酸结合方式是脱水缩合:一个氨基酸分子的羧基(—COOH)与另一个氨基酸分子的氨基(—NH2)相连接，同时脱去一分子水。 
19、DNA与RNA区别 
DNA RNA 
?全称 脱氧核糖核酸 核糖核酸 ?分布 细胞核、线粒体、叶绿体 细胞质 
染色剂 甲基绿 吡罗红 
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链数 双链 单链 碱基 ATCG AUCG 五碳糖 脱氧核糖 核糖 组成单位 脱氧核苷酸 核糖核苷酸 
原核生物、真核生物、噬
代表生物 HIV、SARS病毒 
菌体 
?20、主要能源物质:糖类 
细胞内良好储能物质:脂肪 
人和动物细胞储能物:糖原 
直接能源物质:ATP 
21、糖类: 
?单糖:葡萄糖、果糖、核糖、脱氧核糖 
?二糖:麦芽糖、蔗糖、乳糖 
??多糖:淀粉和纤维素(植物细胞)、糖原(动物细胞) 脂肪:储能;保温;缓冲;减压 
22、脂质: 磷脂:生物膜重要成分 
胆固醇 
固醇: 性激素:促进人和动物生殖器官的发育及生殖细胞形成 维生素D:促进人和动物肠道对Ca和P的吸收 
?23、多糖，蛋白质，核酸等都是生物大分子，基本组成单位依次为:单糖、氨基酸、核苷酸。 
生物大分子以碳链为基本骨架，所以碳是生命的核心元素。 自由水(95.5%):良好溶剂;参与生物化学反应;提供液体环境; 24、水存在形式 运送营养物质及代谢废物 
结合水(4.5%) 
?25、无机盐绝大多数以离子形式存在。哺乳动物血液中Ca2+过低，会出现抽搐症状;患急性肠炎的病人脱水时要补充输入葡萄糖盐水;高温作业大量出汗的工人要多喝淡盐水。 
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 House scaffolding support. Steel in steel processing processing is completed, transport by trucks to the construction site, then H30B perpendicular to the face of the tower crane, artificial binding welded. Concrete by tanker transport to the pier HB60 direct placement of concrete delivery pump, manual open, 38mm shaft for electric plug-in vibrator vibrating compaction. 7.3 7.3.1 in concrete construction of concrete (1) cement-cement construction drawings of buildings according to the requirements, configure the required cement concrete, cement in accordance with existing national and industry standards. Ship each batch of cement factory, on cement quality, factory certificate, review the information for inspection re-inspection. Transport of cement in the transport process, the different varieties and different levels of intensity may not be mixed, and to take measures to prevent the cement from moisture. Storage delivery of cement according to the variety, intensity, the factory lot, bagged or in bulk, respectively, kept in its own warehouses or storage tank to prevent cement deterioration. Bags of cement manufacture date not more than 3 months, bulk cement factory date not more 
26、细胞膜主要由脂质和蛋白质，和少量糖类组成，脂质中磷脂最丰富，功能越复杂的细胞膜，蛋白质种类和数量越多;细胞膜基本支架是磷脂双分子层;细胞膜具有一定的流动性和选择透过性。 
27、细胞膜的功能:控制物质进出细胞，进行细胞间信息交流。 28、植物细胞的细胞壁成分为纤维素和果胶，具有支持和保护作用。
 ?29、制取细胞膜利用哺乳动物成熟红细胞，因为无核膜和细胞器膜。 30、?叶绿体:光合作用的细胞器;双层膜 
?线粒体:有氧呼吸主要场所;双层膜 
核糖体:生产蛋白质的细胞器;无膜 
中心体:与动物细胞有丝分裂有关;无膜 
液泡:调节植物细胞内的渗透压，内有细胞液 
内质网:对蛋白质加工 
高尔基体:对蛋白质加工，分泌 
31、消化酶、抗体等分泌蛋白合成需要四种细胞器:核糖体，内质网、高尔基体、线粒体。 
32、细胞膜、核膜、细胞器膜共同构成细胞的生物膜系统，它们在结构和功能上
维持细胞内环境相对稳定。 紧密联系，协调，
生物膜系统功能:许多重要化学反应的位点吗，把各种细胞器分开，提高生命活动效率。 
核膜:双层膜，其上有核孔，可供mRNA通过核仁 
结构 
33、细胞核 由DNA及蛋白质构成，与染色体是同种物质在不同时 染色质 期的两种状态 
容易被碱性染料染成深色 
功能:是遗传信息库，是细胞代谢和遗传的控制中心 
?34、植物细胞内的液体环境，主要是指液泡中的细胞液。 
原生质层指细胞膜，液泡膜及两层膜之间的细胞质 
植物细胞原生质层相当于一层半透膜;质壁分离中质指原生质层，壁为细胞
壁 
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