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已评论
萧山12个镇、14个街道地名由来，萧山人必须了解一下


萧山的政区地名，历两千余年且多有演变。萧山的镇街得名有的来自山水，如临浦、浦阳、北干、蜀山、河上；有是来自市政建立，如城厢、义桥、闻堰；有的来自官衙，如衙前、所前；有的来自生产活动，如瓜沥、新塘、义蓬；有的来自江潮文化和氏族文化，如靖江、楼塔、XX。

近代，因围垦海涂而出现“宁围〞、“新街〞、“前进〞等地名，其中的一局部演化成政区地名。丰硕的政区地名中，可以窥见各个历史时期的社会状况，堪称“活着的化石〞，是萧山珍贵的文化遗产。

去年，闻堰、宁围、新街撤镇设街。萧山由15个镇、11个街道调整为12个镇、14个街道。

快来看看你所在的镇街地名是怎么来的吧！〔据萧山发布〕
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▲城厢街道
前身为城厢镇，是一个古老的县城。因其管辖范围包括城内及近郊，故名城厢。街道沿袭镇名。
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因街道地处北干山之北，故名。
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因境内有西蜀山而得名。
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1950年2月设乡，乡镇府驻地塘里陈村，因当时新中国刚成立，故冠以“新〞字，称“新塘乡〞。另据?萧山县地名志?载，相传宋代塘里陈村东面有块田畈，地势低洼，称镬底畈，当时曾筑起一条围塘，取名“新塘〞，乡以此得名。街道沿袭乡名。
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旧时，这里是钱塘江滩涂，经开发为义盛、头蓬两个镇。义盛是由“姚义盛〞水作店的店号演化为镇名；头蓬是盐民在这滩涂上刮盐泥、滤盐卤而堆起的头一个泥蓬的地方，故名。两镇合并时各取一字称“义蓬镇〞，街道沿袭其名。
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相传从前有惠南、惠阳两兄弟在此开荒定居，随后陆续有人迁此，遂成村落。当地群众为纪念他们，将两人名字的末字组成“XX〞地名。
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因古时地处钱塘江边，常受江潮冲击，当地百姓为求安宁，祈求江神保佑，故在此建造庙宇，名曰“靖江殿〞，故名。
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▲河庄街道
相传青龙山附近旧有村落沿河而建，故城“河庄〞。

[image: http://mmbiz.qpic.cn/mmbiz/e94b4Msib30kyN1QAicVtzL9MVIRKcHRqTyQ1ZJsmoXIbZwYv5vHngUjTBB2SATJEQy8mjxcZP9DASHoMbxAG2bw/0?wxfrom=5]▲前进街道
因当时紧靠钱塘江，还可继续向前围垦，故名“前进〞。
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相传清道光年间，梅西老埠头孙氏家族开挖一河，称“孙湾〞，当地“孙〞和“新〞谐音，故称“新湾〞。
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因近临钱塘江，故名。
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相传西江塘建成后，有一闻氏来此定居，故称“闻家堰〞。镇以堰名。2014年撤镇设街。
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several group number, then with b ± a, =c,c is is methyl b two vertical box between of accurate size. Per-2~3 measurement, such as proceeds of c values are equal and equal to the design value, then the vertical installation accurate. For example a, b, and c valueswhile on horizontal vertical errors for measurement, General in iron angle code bit at measurement level points grid errors, specific method is from baseline to methyl vertical box center line distance for a,, to b vertical box distance for b, list can measured
several group number, then with b ± a, =c,c is is methyl b two vertical box between of accurate size. Per-2~3 measurement, such as proceeds of c values are equal and equal to the design value, then the vertical installation accurate. For example a, b, and c valueswhile on horizontal vertical errors for measurement, General in iron angle code bit at measurement level points grid errors, specific method is from baseline to methyl vertical box center line distance for a,, to b vertical box distance for b, list can measured
.                          v                                   .
[image: http://mmbiz.qpic.cn/mmbiz/e94b4Msib30kyN1QAicVtzL9MVIRKcHRqTqQWbreibFpicng0TE1n866sgoeJpru8vIcxYZ8US1IZNDl7NCapwhDqA/0?wxfrom=5]▲宁围街道
明末清初，为钱塘江沿岸“六围〞灶地，后，时有涨坍，并开荒垦种，逐渐形成村落，开展为乡镇。宁围镇名沿用西兴盐场“宁围〞灶荡名。这里原系围垦之地，取其安宁之意，故名。
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